### `get_inventory`

Retrieve the inventory for a device. If you call this without any
parameters then you will only get part of the inventory. This is
because a lot of devices nest each component, for instance you may
initially have the chassis, within this the ports - 1 being an sfp
cage, then the sfp itself. The way this API call is designed is to
enable a recursive lookup. The first call will retrieve the root
entry, included within this response will be entPhysicalIndex, you can
then call for entPhysicalContainedIn which will then return the next
layer of results.  To retrieve all items together, see
[get_inventory_for_device](#get_inventory_for_device).

Route: `/api/v0/inventory/:hostname`

- hostname can be either the device hostname or the device id

Input:

- entPhysicalClass: This is used to restrict the class of the
  inventory, for example you can specify chassis to only return items
  in the inventory that are labelled as chassis.
- entPhysicalContainedIn: This is used to retrieve items within the
  inventory assigned to a previous component, for example specifying
  the chassis (entPhysicalIndex) will retrieve all items where the
  chassis is the parent.

Example:

```curl
curl -H 'X-Auth-Token: YOURAPITOKENHERE' https://foo.example/api/v0/inventory/localhost?entPhysicalContainedIn=65536
```

Output:

```json
{
    "status": "ok",
    "message": "",
    "count": 1,
    "inventory": [
        {
            "entPhysical_id": "2",
            "device_id": "32",
            "entPhysicalIndex": "262145",
            "entPhysicalDescr": "Linux 3.3.5 ehci_hcd RB400 EHCI",
            "entPhysicalClass": "unknown",
            "entPhysicalName": "1:1",
            "entPhysicalHardwareRev": "",
            "entPhysicalFirmwareRev": "",
            "entPhysicalSoftwareRev": "",
            "entPhysicalAlias": "",
            "entPhysicalAssetID": "",
            "entPhysicalIsFRU": "false",
            "entPhysicalModelName": "0x0002",
            "entPhysicalVendorType": "zeroDotZero",
            "entPhysicalSerialNum": "rb400_usb",
            "entPhysicalContainedIn": "65536",
            "entPhysicalParentRelPos": "-1",
            "entPhysicalMfgName": "0x1d6b",
            "ifIndex": "0"
        }
    ]
}
```

### `get_inventory_for_device`

Retrieve the flattened inventory for a device.  This retrieves all
inventory items for a device regardless of their structure, and may be
more useful for devices with with nested components.

Route: `/api/v0/inventory/:hostname/all`

- hostname can be either the device hostname or the device id

Example:

```curl
curl -H 'X-Auth-Token: YOURAPITOKENHERE' https://foo.example/api/v0/inventory/localhost?entPhysicalContainedIn=65536
```

Output:

```json
{
    "status": "ok",
    "message": "",
    "count": 1,
    "inventory": [
        {
            "entPhysical_id": "2",
            "device_id": "32",
            "entPhysicalIndex": "262145",
            "entPhysicalDescr": "Linux 3.3.5 ehci_hcd RB400 EHCI",
            "entPhysicalClass": "unknown",
            "entPhysicalName": "1:1",
            "entPhysicalHardwareRev": "",
            "entPhysicalFirmwareRev": "",
            "entPhysicalSoftwareRev": "",
            "entPhysicalAlias": "",
            "entPhysicalAssetID": "",
            "entPhysicalIsFRU": "false",
            "entPhysicalModelName": "0x0002",
            "entPhysicalVendorType": "zeroDotZero",
            "entPhysicalSerialNum": "rb400_usb",
            "entPhysicalContainedIn": "65536",
            "entPhysicalParentRelPos": "-1",
            "entPhysicalMfgName": "0x1d6b",
            "ifIndex": "0"
        }
    ]
}
```
